The firewall is connected in a test lab to another firewall using a 192.168.99.0/24 IP address, and the VLAN99 interface which uses the same IP pool is still enabled. Note: the VLAN99 interface is enabled but the status is down:  
A screenshot of a computer

Description automatically generated with medium confidence

* No connection to the Internet:  
  Graphical user interface, text, application

  Description automatically generated
* The VLAN99 interface cannot be disabled while the WAN1 interface is still connected:  
  A screenshot of a computer

  Description automatically generated
* After physically disconnecting the WAN1 port, the VLAN99 interface can now be disabled:  
  A screenshot of a computer

  Description automatically generated
* After plugging in WAN1 again, now we have a connection to the Internet again, too:  
  Graphical user interface, text, application

  Description automatically generated