Copyright (c) 1992-2020 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
FreeBSD is a registered trademark of The FreeBSD Foundation.
FreeBSD 11.3-STABLE #236 21cbb70bbd1(RELENG_2_4_5): Tue Mar 24 15:26:53 EDT 2020
    root@buildbot1-nyi.netgate.com:/build/ce-crossbuild-245/obj/amd64/YNx4Qq3j/build/ce-crossbuild-245/sources/FreeBSD-src/sys/pfSense amd64
FreeBSD clang version 8.0.1 (tags/RELEASE_801/final 366581) (based on LLVM 8.0.1)
VT(efifb): resolution 1280x1024
CPU: Intel(R) Atom(TM) CPU C3758 @ 2.20GHz (2200.07-MHz K8-class CPU)
  Origin="GenuineIntel"  Id=0x506f1  Family=0x6  Model=0x5f  Stepping=1
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0x4ff8ebbf<SSE3,PCLMULQDQ,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,SDBG,CX16,xTPR,PDCM,SSE4.1,SSE4.2,x2APIC,MOVBE,POPCNT,TSCDLT,AESNI,XSAVE,OSXSAVE,RDRAND>
  AMD Features=0x2c100800<SYSCALL,NX,Page1GB,RDTSCP,LM>
  AMD Features2=0x101<LAHF,Prefetch>
  Structured Extended Features=0x2294e283<FSGSBASE,TSCADJ,SMEP,ERMS,NFPUSG,MPX,PQE,RDSEED,SMAP,CLFLUSHOPT,PROCTRACE,SHA>
  Structured Extended Features3=0x2c000000<IBPB,STIBP,ARCH_CAP>
  XSAVE Features=0xf<XSAVEOPT,XSAVEC,XINUSE,XSAVES>
  IA32_ARCH_CAPS=0x1<RDCL_NO>
  VT-x: (disabled in BIOS) PAT,HLT,MTF,PAUSE,EPT,UG,VPID,VID,PostIntr
  TSC: P-state invariant, performance statistics
real memory  = 8589934592 (8192 MB)
avail memory = 8181899264 (7802 MB)
Event timer "LAPIC" quality 600
ACPI APIC Table: <INTEL  TIANO   >
WARNING: L1 data cache covers less APIC IDs than a core
0 < 1
FreeBSD/SMP: Multiprocessor System Detected: 8 CPUs
FreeBSD/SMP: 1 package(s) x 8 core(s)
ioapic0 <Version 2.0> irqs 0-23 on motherboard
SMP: AP CPU #7 Launched!
SMP: AP CPU #1 Launched!
SMP: AP CPU #2 Launched!
SMP: AP CPU #6 Launched!
SMP: AP CPU #3 Launched!
SMP: AP CPU #5 Launched!
SMP: AP CPU #4 Launched!
Timecounter "TSC-low" frequency 1100035032 Hz quality 1000
random: entropy device external interface
ipw_monitor: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_monitor: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_monitor_fw, 0xffffffff806a2080, 0) error 1
iwi_bss: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_bss: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_bss_fw, 0xffffffff806c9140, 0) error 1
iwi_ibss: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_ibss: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_ibss_fw, 0xffffffff806c91f0, 0) error 1
iwi_monitor: You need to read the LICENSE file in /usr/share/doc/legal/intel_iwi.LICENSE.
iwi_monitor: If you agree with the license, set legal.intel_iwi.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (iwi_monitor_fw, 0xffffffff806c92a0, 0) error 1
wlan: mac acl policy registered
ipw_bss: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_bss: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_bss_fw, 0xffffffff806a1f20, 0) error 1
ipw_ibss: You need to read the LICENSE file in /usr/share/doc/legal/intel_ipw.LICENSE.
ipw_ibss: If you agree with the license, set legal.intel_ipw.license_ack=1 in /boot/loader.conf.
module_register_init: MOD_LOAD (ipw_ibss_fw, 0xffffffff806a1fd0, 0) error 1
kbd0 at kbdmux0
000.000022 [4213] netmap_init               netmap: loaded module
module_register_init: MOD_LOAD (vesa, 0xffffffff812c9960, 0) error 19
random: registering fast source Intel Secure Key RNG
random: fast provider: "Intel Secure Key RNG"
mlx5en: Mellanox Ethernet driver 3.5.2 (September 2019)
nexus0
cryptosoft0: <software crypto> on motherboard
padlock0: No ACE support.
acpi0: <SUPERM SMCI--MB> on motherboard
acpi0: Power Button (fixed)
cpu0: <ACPI CPU> on acpi0
cpu1: <ACPI CPU> on acpi0
cpu2: <ACPI CPU> on acpi0
cpu3: <ACPI CPU> on acpi0
cpu4: <ACPI CPU> on acpi0
cpu5: <ACPI CPU> on acpi0
cpu6: <ACPI CPU> on acpi0
cpu7: <ACPI CPU> on acpi0
hpet0: <High Precision Event Timer> iomem 0xfed00000-0xfed003ff on acpi0
Timecounter "HPET" frequency 24000000 Hz quality 950
Event timer "HPET" frequency 24000000 Hz quality 550
atrtc0: <AT realtime clock> port 0x70-0x77 irq 8 on acpi0
atrtc0: Warning: Couldn't map I/O.
atrtc0: registered as a time-of-day clock, resolution 1.000000s
Event timer "RTC" frequency 32768 Hz quality 0
attimer0: <AT timer> port 0x40-0x43,0x50-0x53 irq 0 on acpi0
Timecounter "i8254" frequency 1193182 Hz quality 0
Event timer "i8254" frequency 1193182 Hz quality 100
Timecounter "ACPI-fast" frequency 3579545 Hz quality 900
acpi_timer0: <24-bit timer at 3.579545MHz> port 0x1808-0x180b on acpi0
pcib0: <ACPI Host-PCI bridge> port 0xcf8-0xcff on acpi0
pcib0: _OSC returned error 0x10
pci0: <ACPI PCI bus> on pcib0
pcib1: <ACPI PCI-PCI bridge> at device 6.0 on pci0
pci1: <ACPI PCI bus> on pcib1
pci1: <processor> at device 0.0 (no driver attached)
pcib2: <ACPI PCI-PCI bridge> mem 0xdf440000-0xdf45ffff at device 9.0 on pci0
pci2: <ACPI PCI bus> on pcib2
pcib3: <ACPI PCI-PCI bridge> mem 0xdf420000-0xdf43ffff at device 16.0 on pci0
pci3: <ACPI PCI bus> on pcib3
pcib4: <ACPI PCI-PCI bridge> mem 0xdf400000-0xdf41ffff at device 17.0 on pci0
pci4: <ACPI PCI bus> on pcib4
pcib5: <ACPI PCI-PCI bridge> at device 0.0 on pci4
pci5: <ACPI PCI bus> on pcib5
vgapci0: <VGA-compatible display> port 0xd000-0xd07f mem 0xde000000-0xdeffffff,0xdf000000-0xdf01ffff at device 0.0 on pci5
ahci0: <Intel Denverton AHCI SATA controller> port 0xe090-0xe097,0xe080-0xe083,0xe040-0xe05f mem 0xdf476000-0xdf477fff,0xdf47d000-0xdf47d0ff,0xdf47c000-0xdf47c7ff at device 19.0 on pci0
ahci0: AHCI v1.31 with 8 6Gbps ports, Port Multiplier not supported
ahcich0: <AHCI channel> at channel 0 on ahci0
ahcich1: <AHCI channel> at channel 1 on ahci0
ahcich2: <AHCI channel> at channel 2 on ahci0
ahcich3: <AHCI channel> at channel 3 on ahci0
ahcich4: <AHCI channel> at channel 4 on ahci0
ahcich5: <AHCI channel> at channel 5 on ahci0
ahcich6: <AHCI channel> at channel 6 on ahci0
ahcich7: <AHCI channel> at channel 7 on ahci0
ahciem0: <AHCI enclosure management bridge> on ahci0
ahci1: <Intel Denverton AHCI SATA controller> port 0xe070-0xe077,0xe060-0xe063,0xe020-0xe03f mem 0xdf474000-0xdf475fff,0xdf47b000-0xdf47b0ff,0xdf47a000-0xdf47a7ff at device 20.0 on pci0
ahci1: AHCI v1.31 with 4 6Gbps ports, Port Multiplier not supported
ahcich11: <AHCI channel> at channel 3 on ahci1
ahcich12: <AHCI channel> at channel 4 on ahci1
ahcich13: <AHCI channel> at channel 5 on ahci1
ahcich14: <AHCI channel> at channel 6 on ahci1
ahciem1: <AHCI enclosure management bridge> on ahci1
xhci0: <Intel Denverton USB 3.0 controller> mem 0xdf460000-0xdf46ffff at device 21.0 on pci0
xhci0: 32 bytes context size, 64-bit DMA
usbus0 on xhci0
usbus0: 5.0Gbps Super Speed USB v3.0
pcib6: <ACPI PCI-PCI bridge> at device 22.0 on pci0
pci6: <ACPI PCI bus> on pcib6
ix0: <Intel(R) PRO/10GbE PCI-Express Network Driver, Version - 3.2.12-k> mem 0xddc00000-0xdddfffff,0xdde04000-0xdde07fff at device 0.0 on pci6
ix0: Using MSI-X interrupts with 9 vectors
ix0: Ethernet address: ac:1f:6b:49:64:b4
ix0: netmap queues/slots: TX 8/2048, RX 8/2048
ix1: <Intel(R) PRO/10GbE PCI-Express Network Driver, Version - 3.2.12-k> mem 0xdda00000-0xddbfffff,0xdde00000-0xdde03fff at device 0.1 on pci6
ix1: Using MSI-X interrupts with 9 vectors
ix1: Ethernet address: ac:1f:6b:49:64:b5
ix1: netmap queues/slots: TX 8/2048, RX 8/2048
pcib7: <ACPI PCI-PCI bridge> at device 23.0 on pci0
pci7: <ACPI PCI bus> on pcib7
ix2: <Intel(R) PRO/10GbE PCI-Express Network Driver, Version - 3.2.12-k> mem 0xdd600000-0xdd7fffff,0xdd804000-0xdd807fff at device 0.0 on pci7
ix2: Using MSI-X interrupts with 9 vectors
ix2: Ethernet address: ac:1f:6b:49:64:b6
ix2: netmap queues/slots: TX 8/2048, RX 8/2048
ix3: <Intel(R) PRO/10GbE PCI-Express Network Driver, Version - 3.2.12-k> mem 0xdd400000-0xdd5fffff,0xdd800000-0xdd803fff at device 0.1 on pci7
ix3: Using MSI-X interrupts with 9 vectors
ix3: Ethernet address: ac:1f:6b:49:64:b7
ix3: netmap queues/slots: TX 8/2048, RX 8/2048
pci0: <simple comms> at device 24.0 (no driver attached)
isab0: <PCI-ISA bridge> at device 31.0 on pci0
isa0: <ISA bus> on isab0
pci0: <memory> at device 31.2 (no driver attached)
pci0: <serial bus> at device 31.5 (no driver attached)
uart1: <16550 or compatible> port 0x2f8-0x2ff irq 3 on acpi0
ppc0: cannot reserve I/O port range
est0: <Enhanced SpeedStep Frequency Control> on cpu0
est1: <Enhanced SpeedStep Frequency Control> on cpu1
est2: <Enhanced SpeedStep Frequency Control> on cpu2
est3: <Enhanced SpeedStep Frequency Control> on cpu3
est4: <Enhanced SpeedStep Frequency Control> on cpu4
est5: <Enhanced SpeedStep Frequency Control> on cpu5
est6: <Enhanced SpeedStep Frequency Control> on cpu6
est7: <Enhanced SpeedStep Frequency Control> on cpu7
ZFS filesystem version: 5
ZFS storage pool version: features support (5000)
Timecounters tick every 1.000 msec
ugen0.1: <0x8086 XHCI root HUB> at usbus0
uhub0: <0x8086 XHCI root HUB, class 9/0, rev 3.00/1.00, addr 1> on usbus0
uhub0: 8 ports with 8 removable, self powered
ugen0.2: <American Power Conversion Back-UPS XS 950U   FW925.T2 .I USB FWT2> at usbus0
ugen0.3: <Logitech USB Keyboard> at usbus0
ukbd0 on uhub0
ukbd0: <USB Keyboard> on usbus0
kbd1 at ukbd0
uhid0 on uhub0
uhid0: <USB Keyboard> on usbus0
ugen0.4: <vendor 0x05e3 USB2.0 Hub> at usbus0
uhub1 on uhub0
uhub1: <vendor 0x05e3 USB2.0 Hub, class 9/0, rev 2.00/32.98, addr 3> on usbus0
uhub1: MTT enabled
uhub1: 4 ports with 4 removable, self powered
ugen0.5: <vendor 0x0557 product 0x7000> at usbus0
uhub2 on uhub1
uhub2: <vendor 0x0557 product 0x7000, class 9/0, rev 2.00/0.00, addr 4> on usbus0
uhub2: 4 ports with 3 removable, self powered
ugen0.6: <vendor 0x0557 product 0x2419> at usbus0
ukbd1 on uhub2
ukbd1: <vendor 0x0557 product 0x2419, class 0/0, rev 1.10/1.00, addr 5> on usbus0
kbd2 at ukbd1
ugen0.7: <vendor 0x05e3 USB2.0 Hub> at usbus0
uhub3 on uhub1
uhub3: <vendor 0x05e3 USB2.0 Hub, class 9/0, rev 2.00/32.98, addr 6> on usbus0
uhub3: MTT enabled
uhub3: 4 ports with 4 removable, self powered
ses0 at ahciem0 bus 0 scbus8 target 0 lun 0
ses0: <AHCI SGPIO Enclosure 2.00 0001> SEMB S-E-S 2.00 device
ses0: SEMB SES Device
ses1 at ahciem1 bus 0 scbus13 target 0 lun 0
ses1: <AHCI SGPIO Enclosure 2.00 0001> SEMB S-E-S 2.00 device
ses1: SEMB SES Device
ada0 at ahcich12 bus 0 scbus10 target 0 lun 0
ada0: <KINGSTON SA400S37120G SBFKJ1A3> ACS-3 ATA SATA 3.x device
ada0: Serial Number 50026B76836116DD
ada0: 600.000MB/s transfers (SATA 3.x, UDMA6, PIO 512bytes)
ada0: Command Queueing enabled
ada0: 114473MB (234441648 512 byte sectors)
ses1: pass1,ada0 in 'Slot 04', SATA Slot: scbus10 target 0
Trying to mount root from zfs:zroot/ROOT/default []...
random: unblocking device.
CPU: Intel(R) Atom(TM) CPU C3758 @ 2.20GHz (2200.07-MHz K8-class CPU)
  Origin="GenuineIntel"  Id=0x506f1  Family=0x6  Model=0x5f  Stepping=1
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0x4ff8ebbf<SSE3,PCLMULQDQ,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,SDBG,CX16,xTPR,PDCM,SSE4.1,SSE4.2,x2APIC,MOVBE,POPCNT,TSCDLT,AESNI,XSAVE,OSXSAVE,RDRAND>
  AMD Features=0x2c100800<SYSCALL,NX,Page1GB,RDTSCP,LM>
  AMD Features2=0x101<LAHF,Prefetch>
  Structured Extended Features=0x2294e283<FSGSBASE,TSCADJ,SMEP,ERMS,NFPUSG,MPX,PQE,RDSEED,SMAP,CLFLUSHOPT,PROCTRACE,SHA>
  Structured Extended Features3=0xac000400<MD_CLEAR,IBPB,STIBP,ARCH_CAP,SSBD>
  XSAVE Features=0xf<XSAVEOPT,XSAVEC,XINUSE,XSAVES>
  IA32_ARCH_CAPS=0x69<RDCL_NO,SKIP_L1DFL_VME,MDS_NO>
  VT-x: (disabled in BIOS) PAT,HLT,MTF,PAUSE,EPT,UG,VPID,VID,PostIntr
  TSC: P-state invariant, performance statistics
padlock0: No ACE support.
aesni0: <AES-CBC,AES-XTS,AES-GCM,AES-ICM> on motherboard
lo0: link state changed to UP
ix2: link state changed to UP
tun2: changing name to 'ovpns2'
ovpns2: link state changed to UP
tun1: changing name to 'ovpns1'
ovpns1: link state changed to UP
pflog0: promiscuous mode enabled
ix1: link state changed to UP
ix3: link state changed to UP
ix3: promiscuous mode enabled
ix2: promiscuous mode enabled
ix1: link state changed to DOWN
ugen0.3: <Logitech USB Keyboard> at usbus0 (disconnected)
ukbd0: at uhub0, port 2, addr 2 (disconnected)
ukbd0: detached
uhid0: at uhub0, port 2, addr 2 (disconnected)
uhid0: detached