
NanoBSD Firmware upgrade in progress...

Installing /root/latest.tgz.
SLICE         2
OLDSLICE      1
TOFLASH       vtbd0s2
COMPLETE_PATH vtbd0s2a
GLABEL_SLICE  pfsense1
Fri Apr 22 08:38:09 UTC 2016

total 4
dr-xr-xr-x  25 root  wheel      512B Apr 22 03:36 .
drwxr-xr-x  25 root  wheel      512B Apr 22 03:36 ..
crw-r--r--   1 root  wheel      0x22 Apr 22 08:36 acpi
crw-rw-r--   1 root  operator   0x24 Apr 22 08:36 apm
crw-rw----   1 root  operator   0x23 Apr 22 08:36 apmctl
crw-------   1 root  wheel      0x43 Apr 22 08:36 atkbd0
crw-------   1 root  kmem       0x14 Apr 22 08:36 audit
crw-------   1 root  wheel      0x20 Apr 22 03:36 bpf
lrwxr-xr-x   1 root  wheel        3B Apr 22 08:36 bpf0 -> bpf
crw-------   1 root  wheel       0x6 Apr 22 08:37 console
crw-------   1 root  wheel      0x42 Apr 22 08:36 consolectl
crw-rw-rw-   1 root  wheel      0x49 Apr 22 03:36 crypto
crw-rw-rw-   1 root  wheel      0x1c Apr 22 08:36 ctty
crw-rw----   1 uucp  dialer     0x29 Apr 22 08:36 cuau0
crw-rw----   1 uucp  dialer     0x2a Apr 22 08:36 cuau0.init
crw-rw----   1 uucp  dialer     0x2b Apr 22 08:36 cuau0.lock
crw-rw----   1 uucp  dialer     0x2f Apr 22 08:36 cuau1
crw-rw----   1 uucp  dialer     0x30 Apr 22 08:36 cuau1.init
crw-rw----   1 uucp  dialer     0x31 Apr 22 08:36 cuau1.lock
crw-------   1 root  wheel       0x5 Apr 22 08:36 devctl
cr--r--r--   1 root  wheel      0x25 Apr 22 08:36 devstat
dr-xr-xr-x   2 root  wheel      512B Apr 22 08:36 fd
crw-------   1 root  wheel      0x1f Apr 22 08:36 fido
crw-r-----   1 root  operator    0x3 Apr 22 08:36 geom.ctl
crw-------   1 root  wheel      0x18 Apr 22 08:36 io
lrwxr-xr-x   1 root  wheel        6B Apr 22 08:36 kbd0 -> atkbd0
lrwxr-xr-x   1 root  wheel        7B Apr 22 08:36 kbd1 -> kbdmux0
crw-------   1 root  wheel      0x1a Apr 22 03:36 kbdmux0
crw-------   1 root  wheel      0x17 Apr 22 08:36 klog
crw-r-----   1 root  kmem       0x1e Apr 22 08:36 kmem
crw-r-----   1 root  operator   0x4e Apr 22 03:36 md0
crw-r-----   1 root  operator   0x52 Apr 22 03:36 md1
crw-------   1 root  wheel      0x4c Apr 22 08:36 mdctl
crw-r-----   1 root  kmem       0x1d Apr 22 08:36 mem
crw-rw-rw-   1 root  wheel      0x15 Apr 22 08:36 midistat
crw-------   1 root  kmem       0x13 Apr 22 08:36 nfslock
crw-rw-rw-   1 root  wheel       0x7 Apr 22 08:38 null
crw-r--r--   1 root  wheel       0x9 Apr 22 08:36 pci
crw-rw----   1 root  proxy      0x48 Apr 22 08:36 pf
crw-rw-rw-   1 root  wheel       0xa Apr 22 08:36 ptmx
crw-rw-rw-   1 root  wheel       0xb Apr 22 03:36 random
cr--r--r--   1 root  wheel       0x4 Apr 22 08:36 sndstat
crw-------   1 root  wheel      0x19 Apr 22 03:36 speaker
lrwxr-xr-x   1 root  wheel        4B Apr 22 08:36 stderr -> fd/2
lrwxr-xr-x   1 root  wheel        4B Apr 22 08:36 stdin -> fd/0
lrwxr-xr-x   1 root  wheel        4B Apr 22 08:36 stdout -> fd/1
crw-------   1 root  wheel      0x16 Apr 22 08:36 sysmouse
crw-------   1 root  wheel      0x26 Apr 22 08:37 ttyu0
crw-------   1 root  wheel      0x27 Apr 22 08:36 ttyu0.init
crw-------   1 root  wheel      0x28 Apr 22 08:36 ttyu0.lock
crw-------   1 root  wheel      0x2c Apr 22 08:36 ttyu1
crw-------   1 root  wheel      0x2d Apr 22 08:36 ttyu1.init
crw-------   1 root  wheel      0x2e Apr 22 08:36 ttyu1.lock
crw-------   1 root  wheel      0x32 Apr 22 08:37 ttyv0
crw-------   1 root  wheel      0x33 Apr 22 08:36 ttyv1
crw-------   1 root  wheel      0x34 Apr 22 08:36 ttyv2
crw-------   1 root  wheel      0x35 Apr 22 08:36 ttyv3
crw-------   1 root  wheel      0x36 Apr 22 08:36 ttyv4
crw-------   1 root  wheel      0x37 Apr 22 08:36 ttyv5
crw-------   1 root  wheel      0x38 Apr 22 08:36 ttyv6
crw-------   1 root  wheel      0x39 Apr 22 08:36 ttyv7
crw-------   1 root  wheel      0x3a Apr 22 08:36 ttyv8
crw-------   1 root  wheel      0x3b Apr 22 08:36 ttyv9
crw-------   1 root  wheel      0x3c Apr 22 08:36 ttyva
crw-------   1 root  wheel      0x3d Apr 22 08:36 ttyvb
crw-------   1 root  wheel      0x3e Apr 22 08:36 ttyvc
crw-------   1 root  wheel      0x3f Apr 22 08:36 ttyvd
crw-------   1 root  wheel      0x40 Apr 22 08:36 ttyve
crw-------   1 root  wheel      0x41 Apr 22 08:36 ttyvf
dr-xr-xr-x   2 root  wheel      512B Apr 22 08:36 ufs
crw-------   1 root  wheel      0x45 Apr 22 08:36 ufssuspend
lrwxr-xr-x   1 root  wheel        6B Apr 22 08:36 urandom -> random
crw-r--r--   1 root  operator   0x4a Apr 22 08:36 usbctl
crw-r-----   1 root  operator   0x4d Apr 22 08:36 vtbd0
crw-r-----   1 root  operator   0x4f Apr 22 08:36 vtbd0s1
crw-r-----   1 root  operator   0x55 Apr 22 08:36 vtbd0s1a
crw-r-----   1 root  operator   0x50 Apr 22 08:36 vtbd0s2
crw-r-----   1 root  operator   0x56 Apr 22 08:36 vtbd0s2a
crw-r-----   1 root  operator   0x51 Apr 22 08:36 vtbd0s3
crw-------   1 root  operator   0x4b Apr 22 08:36 xpt0
crw-rw-rw-   1 root  wheel       0x8 Apr 22 08:36 zero

-rw-r--r--  1 root  wheel   171M Apr 22 08:38 /root/latest.tgz

MD5 (/root/latest.tgz) = 48290c70e02309cffb05d7abe0c286ea

/dev/ufs/pfsense0 on / (ufs, local, noatime, synchronous)
devfs on /dev (devfs, local)
/dev/ufs/cf on /cf (ufs, local, noatime, synchronous)
/dev/md0 on /tmp (ufs, local)
/dev/md1 on /var (ufs, local)
devfs on /var/dhcpd/dev (devfs, local)

last pid: 49917;  load averages:  0.79,  0.35,  0.14  up 0+00:01:35    08:38:10
32 processes:  1 running, 31 sleeping

Mem: 50M Active, 218M Inact, 79M Wired, 15M Buf, 116M Free
Swap: 


  PID USERNAME  THR PRI NICE   SIZE    RES STATE   C   TIME    WCPU COMMAND
  292 root        1  52    0   213M 43416K accept  1   0:04   5.96% php-fpm
26796 root        1  20    0 44596K  6992K kqread  1   0:00   0.00% lighttpd
  290 root        1  52    0   212M 42360K accept  0   0:00   0.00% php-fpm
  291 root        1  22    0   208M 40104K accept  0   0:00   0.00% php-fpm
13798 root        1  20    0 16804K  2312K bpf     1   0:00   0.00% filterlog
21271 unbound     2  20    0 42940K 13944K kqread  1   0:00   0.00% unbound
92924 root        2  20    0 28344K 18120K usem    1   0:00   0.00% ntpd
78414 root        1  20    0 14640K  2380K select  1   0:00   0.00% syslogd
22841 root        1  20    0 12456K  2184K select  1   0:00   0.00% apinger
  289 root        1  20    0   204M 22148K kqread  0   0:00   0.00% php-fpm
41959 root        1  52    0 17136K  2792K wait    0   0:00   0.00% sh
  322 root        1  20    0 13160K  4388K select  1   0:00   0.00% devd
  306 root        1  40   20 19024K  2536K kqread  0   0:00   0.00% check_reload_status
27235 root        1  52   20 17136K  2680K wait    0   0:00   0.00% sh
22861 root        1  20    0 28328K  2984K piperd  1   0:00   0.00% rrdtool
13811 root        1  39    0 12556K  2188K select  1   0:00   0.00% dhcp6c
86894 root        2  39    0 14748K  2276K nanslp  0   0:00   0.00% sshlockout_pf
16974 root        1  20    0 18780K  2316K select  0   0:00   0.00% inetd



NanoBSD upgrade starting


dd if=/dev/zero of=/dev/vtbd0s2 bs=1m count=1
1+0 records in
1+0 records out
1048576 bytes transferred in 0.004193 secs (250073720 bytes/sec)

/usr/bin/gzip -dc /root/latest.tgz | /bin/dd of=/dev/vtbd0s2 obs=64k
3844449+0 records in
30034+1 records out
1968357888 bytes transferred in 10.594886 secs (185783771 bytes/sec)
After upgrade fdisk/bsdlabel

/sbin/fsck_ufs -y /dev/vtbd0s2a
** /dev/vtbd0s2a
** Last Mounted on /builder/pfsense-230/tmp/pfSense/_.mnt
** Phase 1 - Check Blocks and Sizes
** Phase 2 - Check Pathnames
** Phase 3 - Check Connectivity
** Phase 4 - Check Reference Counts
** Phase 5 - Check Cyl groups
15850 files, 964552 used, 2815476 free (2380 frags, 351637 blocks, 0.1% fragmentation)

***** FILE SYSTEM IS CLEAN *****

/sbin/tunefs -L pfsense1 /dev/vtbd0s2a
Checking for post_upgrade_command...

/dev/ufs/pfsense1 / ufs ro,sync,noatime 1 1
/dev/ufs/cf /cf ufs ro,sync,noatime 1 1



gpart set -a active -i 2 vtbd0
active set on vtbd0s2

/usr/sbin/boot0cfg -s 2 -v /dev/vtbd0
#   flag     start chs   type       end chs       offset         size
1   0x00      0:  1: 1   0xa5    741: 15:63           63      3844449
2   0x80    742:  1: 1   0xa5    459: 15:63      3844575      3844449
3   0x00    460:  0: 1   0xa5    561: 15:63      7689024       102816

version=2.0  drive=0x80  mask=0x3  ticks=182  bell=# (0x23)
options=packet,update,nosetdrv
volume serial ID 9090-9090
default_selection=F2 (Slice 2)
Fri Apr 22 08:38:21 UTC 2016

